# School Transportation Vehicle (School Bus) Pre-Trip and Post Trip Requirements (STU 9)

**2021-2022**

**ALL ITEMS ON THIS CHECKLIST ARE MANDATORY. USE OF THIS SPECIFIC CHECKLIST IS NOT MANDATORY.**

"Per 1 CCR 301-26, 4204-R-8.02 The pre-trip and post-trip inspection requirements for school transportation vehicles, other than small vehicles, shall include at a minimum all items listed on the CDE School Transportation Vehicle (School Bus) Pre-Trip and Post Trip Requirements (STU-9) Form.”

|  |  |  |  |
| --- | --- | --- | --- |
| ***Front of Vehicle*** | ***Side of Vehicle*** | ***In Cab*** | ***Passenger Items*** |
| Light Lens Condition | Light Lens Condition | Safety Belt | Steps |
| ***Engine Compartment*** | Reflectors | Fire Extinguisher | Handrail |
| Oil Level | ***Driver/Fuel Area*** | Electrical Fuses | Step Light |
| Coolant Level | Door | Triangles | Lift |
| Power Steering Fluid | Mirror | Safe Start | Seating Secured |
| Water Pump | Fuel Tank | ABS |  |
| Belt or Gear | Fuel Leaks | Temperature Gauge | ***Post-Trip*** |
| Alternator | Fuel Cap | Oil Pressure Gauge | Student Check |
| Belt or Gear | ***Under Vehicle*** | Voltmeter Gauge | Walk Around |
| Air Compressor | Drive Shaft | Air Gauge | Articles left on the Bus |
| Belt or Gear | Exhaust System | Left Turn Signal | Open windows/doors |
| Leaks | Frame | Right Turn Signal | Damage Vandalism |
| Hoses | ***Suspension*** | Hazard Lights | Mechanical Problems |
| ***Steering*** | Springs | Headlights | Operational Problems |
| Box | Spring Mount(s) | High Beams |  |
| Hoses | Shock(s) | Horn |  |
| Pitman Arm | U-Bolts | Heater(s) |  |
| Drag Link | Air Bag | Defroster |  |
| ***Front/Rear Brakes*** | Air Bag Mount | Mirrors |  |
| Slack Adjustor | ***Wheels*** | Windshield |  |
| Brake Chamber | Rim | Wipers |  |
| Brake Hose or Line | Lug Nuts | Washers |  |
| Drum or Disk | Axle Hub Oil Seal | Parking Brake |  |
| Linings or Pads | Spacers | Service Brake |  |
| ***Tires*** | ***Rear of Vehicle*** | Dome Lights |  |
| Inflation | Light Lens Condition | Emergency Door Alarm |  |
| Condition | Reflectors | Emergency Window Alarm |  |
| Depth | Splash Guard | Emergency Kit |  |
| ***Exterior Lights*** | Emergency Door | Body Fluid Kit |  |
| Clearance | ***Air Brake Check*** | Seat Belt Cutter |  |
| Hazard | \*1 Compressor | Student Mirror |  |
| Turn Signals | \*2 System Leaks | Communications |  |
| Overhead Amber | \*3 Low Air Warning |  |  |
| Overhead Red | \*4 Valve Set or Hydraulic Brake Check |  |  |
| Stop Arm  (including operation) |  |  | \* If No Air Brakes Line Out Components |
| Brake |  |  |  |
| Tail |  |  |  |

